REQUIREMENTS FOR SPECIFICATION OF WASTEWATER TREATMENT PLANT
NAME OF PROJECT:	No :
CUSTOMER	REFERENT
DATE	Klepněte sem a zadejte datum.
LOCATION (STATE, CITY)
Seismic zone	According to AWWA D – 103
Wind Speed	km/h
Snow load	kN/m2
Type of waste water - municipal, breweries, slaughter houses, etc.
Population connected to the sewerage system	Currently
View
Average daily inflow Q24	m3/day
Maximum daily inflow Qd	m3/day
Maximum hourly inflow Qh	m3/hour
Maximum inflow of sewage and rainwater Qmax	m3/hour
Input pollution
CHOD cr	mg/l
BOD 5	mg/l
Suspended solids NL	mg/l
Total Nitrogen ( N)	mg/l
Total Phosphorus P	mg/l
Output paramethers
BOD 5	mg/l
Total Nitrogen ( N)	mg/l
Total Phosphorus P	mg/l
Suspended solids NL	mg/l
Ammoniacal nitrogen NH4+H	mg/l
Nitric nitrogen NO3-	mg/l
Nitrite nitrogen NO2-	mg/l
The required way of handling with sludge
Special customer requirements