REQUIREMENTS FOR SPECIFICATION OF GLASS-COATED STEEL TANK
Name of project:	No. :
INVESTOR	REFERENT
Date	Klepněte sem a zadejte datum.
Location (state, city)
Seismic zone or seismic horizontal acceleration	Ac. to AWWA D – 103 m/s
Wind speed	km/h
POZN.: If not determined other way, the tank will be calculated as a typical, without roof, designed for seismic zone 0 and wind speed 110 km/h.
TYP STAVBY
Tank requirement
Diameter [m]
Height [m], numbers of rows [pcs]
NEtt volume [m3]
Colour of glass-coat
Roof of tank	Zvolte položku.
Roof type
Maximum overpressure [kPa]
Maximum underpressure [kPa]
Snow load	kN/m2
POZN.: Parametres regarding pressure and snow load are required just in case of the tank including roof. If not determined other way, the tank is standard by calculated for atmospheric pressure. The overpressure = 0 kPa.
Requirement for platform and access laders
Requirement for flanges, nozzles
Requirement for technological part (technology)
The part of enquiry is drawing documentation
Specification of medium stored in the tank
Name
Density [kg/m3]
pH + concentration
Chemical and physical parameters
Other information about medium

Statement of Vitkovice design department
Designer
Approved by leader